SUPREMA ACCESS CONTROL DEVICE - BioStation T2 
TECHNICAL SPECIFICATIONS
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PART 1 - GENERAL 
The intent of this document is to specify the minimum criteria for the design, supply, installation, and commissioning of the BioStation T2.
SUMMARY
Section includes a biometric reader and door controller with Ethernet network connectivity.
Product - An IP enabled biometric reader and door controller, capable of scanning and registering cards, managing users and controlling access.

REFERENCE
1. Standards
1. IEEE 802.3 Ethernet Standards
2. FCC - Code of Federal Regulations, Title 47, Part 15, Class B

1.01 SUBMITTALS


QUALIFICATIONS
1. Manufacturer shall be ISO 9001 certified with a minimum of five years’ experience in producing access control equipment.
Installers shall be trained by the Manufacturer to install, configure and commission the access control system.

WARRANTY
1. Manufacturer shall provide a limited (  ) month warranty for the product to be free of defect in material and workmanship.
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PART 2 - PRODUCTS
EQUIPMENT 
1. Manufacturer 
Suprema Inc. 
17F Parkview Office Tower, Jeongja, Bundang, Seongnam, Gyeonggi, 463-863, Republic of Korea
Tel: 82-31-783-4502, Fax: 82-31-783-4503, www.supremainc.com
support@supremainc.com
Model(s): BioStation T2 
Alternates: NONE

DESCRIPTION
1. The biometric reader and door controller (“reader/controller”) shall be an IP-enabled device capable of scanning fingerprints and RFID cards, managing users and controlling access.

FEATURES
1. Face recognition technology
1. NIST MINEX compliant 
1. 5” touchscreen LCD
1. Embedded BioStar Lite web server
1. PoE, Wi-Fi, TCP/IP, RS-485/232, Wiegand, Relay interface
1. Video phone - IP based video and audio interface or analog video phone
1. Built-in card reader (125KHz EM, 13.56MHz MIFARE/DesFire)
1. Intuitive Graphical User Interface (GUI) system

SPECIFICATIONS
	General
	Biometric
	Fingerprint

	
	RF Option
	BST2R-OC: 125kHz EM

	
	
	BST2RW: 125kHz EM

	
	
	BST2M-OC: 13.56MHz MIFARE, MIFARE Plus, DESFire, ISO14443A

	
	
	BST2MW-OC: 13.56MHz MIFARE, MIFARE Plus, DESFire, ISO14443A

	
	Certificates
	CE, FCC, KC, RoHS

	Capacity
	Max. User (1:1)
	200,000

	
	Max. User (1:N)
	10,000

	
	Max. Template (1:1)
	400,000

	
	Max. Template (1:N)
	20,000

	
	Max. Text Log
	1,000,000

	
	Max. Image Log
	5,000

	Interface
	WiFi
	Optional

	
	TCP/IP
	Yes

	
	RS-485
	1ch Host, 1ch Slave

	
	RS-232
	Yes

	
	Wiegand
	1ch In or 1ch Out

	
	Input
	4 Inputs

	
	Relay
	2 Relays

	
	USB
	Host and Slave

	
	SD Card Slot
	Yes

	Mechanical
	CPU
	667MHz RISC + 900MHz DSP

	
	Memory
	256MB RAM + 1GB Flash

	
	LCD
	5" Color Touch

	
	LED Indicator
	Multi-Color

	
	Sound
	16bit Hi-Fi

	
	Operating Temp.
	-20° to 50°C

	
	Tamper
	Yes

	
	PoE
	Yes

	
	Dimensions
	155 x 155 x 40 (WxHxD mm)

	Electrical
	Power
	Min. 10.8 VDC
Typ. 12 VDC
Max. 13.2 VDC

	
	Consumption
	Max. 570 mA

	
	Consumption with USB Wireless LAN
	Max. 1350 mA

	
	Switch Input VIH
	Min. 3.5 V
Max. 10 V

	
	Switch Input VIL
	Max. 2 V

	
	Switch Pull-up Resistor
	4.7 kΩ (The input ports are pulled up with 4.7 kΩ resistors.)

	
	Relay 
	Form C Relay 
Voltage: Max. 24 VDC
Current: Typ. 0.5 A, Max. 1 A

	Platform
	BioStar 1
	Supported
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PART 3 - EXECUTION
INSTALLER
1. Contractor personnel shall comply with all applicable state and local licensing requirements.

PREPARATION
1. Contractor shall avoid locating the reader/controller in a location subject to direct sunlight, dust or soot.
IP addressing shall be coordinated with the Owner’s responsible IT personnel.

STORAGE
1. The system shall be stored in an environment where temperature is in the range of -4 - 122°F (-20 - +50°C).

INSTALLATION
1. All wires shall be run through conduit to prevent failure caused by rodent damage.
Connections between card readers and a door controller shall not exceed 100 meters.
All peripheral devices shall be grounded.

EXAMINATION
1. All network connections to the reader/controller shall be tested for proper levels of performance.
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